Skip to content
Open now — dispatching 24/7 across Oklahoma Call (833) 435-9778 for same-day service

Drains & Sewers · plumbing advice

# Drain Cleaning vs Hydro Jetting: Which One Does Your Line Need?

Cabling and jetting solve different problems. Here's how to tell which your drain needs, and when jetting is the wrong call.

Both clear a blocked line. They do it differently enough that using the wrong one is either a waste of money or a temporary fix that fails again in a month.

## What cabling does

A motorised cable with a cutting head is fed down the line. It bores through the obstruction and, with the right head, cuts roots. Flow returns immediately.

What it does not do is clean the pipe wall. Grease and scale coating the inside of the pipe stay there. You get a hole through the blockage rather than a clean pipe, which is why a cabled grease line often blocks again within weeks or months.

Cabling is the right call for: a single fixture blockage, a solid object, a first-time main line clog, and any line too fragile for high pressure. See drain cleaning.

## What jetting does

A high-pressure hose with rear-facing jets is pulled through the line, scouring the wall back to bare pipe and flushing debris downstream. The line ends up close to its original diameter.

Jetting is the right call for: grease-laden kitchen and restaurant lines, heavy scale in older cast iron, root masses combined with build-up, and any line that has been cabled repeatedly without lasting results. See hydro jetting.

## When jetting is the wrong call

High pressure in a pipe that is already cracked, badly corroded or collapsed can turn a bad line into an open one. This is exactly why a camera should go down first. Any company that jets without inspecting is taking a risk with your line, not theirs.

A camera inspection before jetting takes under an hour and tells you the pipe material, the condition, and whether the real answer is repair rather than cleaning at all.

## A simple rule

First blockage in years, one fixture: cable it. Third blockage in the same line this year: camera it, then jet it if the pipe is sound. Blockage plus a camera showing cracks, offsets or a belly: stop cleaning and fix the pipe.

## Restaurants and commercial kitchens

Grease lines need a maintenance cycle, not emergency callouts. Most Oklahoma kitchens do well jetting every six to twelve months depending on volume. It is scheduled, it happens after closing, and it costs a fraction of an emergency shutdown. See commercial plumbing.

Not sure which yours needs? Call (833) 435-9778 and describe the history. The pattern of blockages usually answers it.

> Need this sorted today? Call (833) 435-9778. We answer 24/7 across Oklahoma, quote a flat price before starting, and charge the same rate at night and on weekends.

## Related reading

Drains & Sewers

### Sewage Smell in the House: Six Causes and How to Find Yours

A sewage smell indoors is never just a smell — it means sewer gas is getting past a barrier. Here's how to track down which one failed.

Read →
Water Heaters

### Tankless vs Tank Water Heater: An Honest Comparison for Oklahoma Homes

Tankless isn't automatically better. Here's where each type wins, and the Oklahoma-specific factors that decide it.

Read →
Water Heaters

### Hot Water Runs Out Fast: Why, and What Actually Fixes It

If your shower goes cold in eight minutes, the tank size is often not the problem. Here's what to check before spending money.

Read →

### Book a plumber near you

- Plumber in Oklahoma City, OK
- Plumber in Tulsa, OK
- Plumber in Norman, OK
- Plumber in Broken Arrow, OK
- Plumber in Edmond, OK
- Plumber in Lawton, OK
- Plumber in Moore, OK
- Plumber in Midwest City, OK
- Plumber in Enid, OK
- Plumber in Stillwater, OK
- Plumber in Owasso, OK
- Plumber in Bartlesville, OK
- All Oklahoma cities →

## Water where it shouldn't be?

Tell us what you're seeing and we'll route the closest plumber to you anywhere in Oklahoma. Price agreed before any work starts.

Call (833) 435-9778
Tap to call (833) 435-9778 — 24/7