Skip to content
Open now — dispatching 24/7 across Oklahoma Call (833) 435-9778 for same-day service

Leaks & Pipes · plumbing advice

# How to Find a Water Leak in Your House (Without Opening Walls)

A step-by-step method for confirming and narrowing down a hidden water leak, using nothing more than your meter and a bit of patience.

Before anyone opens a wall, you want to know two things: whether there is genuinely a leak, and roughly which side of the house it is on. You can establish both yourself.

## Step 1: confirm a leak exists

Turn off every fixture and appliance that uses water — including ice makers, humidifiers and irrigation. Go to the meter and note the reading, or watch the small leak indicator dial. Wait two hours with no water use, then read it again.

Any movement means water is going somewhere. No movement over two hours means you do not have a continuous leak, though you may still have an intermittent one.

## Step 2: inside or outside?

Shut the main valve at the house. Watch the meter again. If it is still moving with the house isolated, the leak is between the meter and the house — a service line problem. If it stops, the leak is inside.

## Step 3: hot side or cold side?

Shut the cold inlet valve on top of the water heater. If the meter stops, the leak is on the hot side. This is a genuinely useful narrowing — hot water lines under a slab fail far more often than cold, and it is a strong pointer toward a slab leak.

## Step 4: look for the physical signs

- A warm patch on the floor — hot line under the slab.
- Persistently damp or unusually green ground in one part of the yard.
- Bubbling paint, soft drywall or a musty smell.
- Cracks appearing in tile, or a floor that has started to lift.
- The sound of running water when everything is off — put an ear to the floor in a quiet house.

## What we do next

With the leak confirmed and the side narrowed down, professional detection uses acoustic listening, line tracing and pressure testing to get within a foot or two. That is the difference between one small access hole and a wall full of exploratory cuts, which is why the detection fee usually pays for itself in drywall alone.

We credit the detection fee against the repair. Call (833) 435-9778 once you have run the meter test — the results tell us a lot before we arrive.

> Need this sorted today? Call (833) 435-9778. We answer 24/7 across Oklahoma, quote a flat price before starting, and charge the same rate at night and on weekends.

## Related reading

Drains & Sewers

### Drain Cleaning vs Hydro Jetting: Which One Does Your Line Need?

Cabling and jetting solve different problems. Here's how to tell which your drain needs, and when jetting is the wrong call.

Read →
Water Heaters

### Brown Water From the Faucet: Is It the Pipes, the Heater or the City?

Rusty or brown tap water has three likely sources. A few quick checks tell you which one, and whether it's safe to use.

Read →
Leaks & Pipes

### Low Water Pressure in the House: 7 Causes, Ranked by Likelihood

Low water pressure in one tap means something different from low pressure everywhere. Here's how Oklahoma plumbers narrow it down before opening a wall.

Read →

### Book a plumber near you

- Plumber in Oklahoma City, OK
- Plumber in Tulsa, OK
- Plumber in Norman, OK
- Plumber in Broken Arrow, OK
- Plumber in Edmond, OK
- Plumber in Lawton, OK
- Plumber in Moore, OK
- Plumber in Midwest City, OK
- Plumber in Enid, OK
- Plumber in Stillwater, OK
- Plumber in Owasso, OK
- Plumber in Bartlesville, OK
- All Oklahoma cities →

## Water where it shouldn't be?

Tell us what you're seeing and we'll route the closest plumber to you anywhere in Oklahoma. Price agreed before any work starts.

Call (833) 435-9778
Tap to call (833) 435-9778 — 24/7